# Addendum #1

**RFP #WRESA-16-2023-2024-03 Parking Light Poles**

## Questions, Answers, and Revisions

**Revision 1: Proposal Due Date has changed from May 8, 2024 by 12:00 pm Eastern Time to May 15, 2024 by 12:00 pm Eastern Time**

**Revision 2:** There will be a non-mandatory on-site visit to view the electrical on May 9, 2024 at 8:30 am Eastern Time in the Parking Lot at the Annex Building off Venoy Road (5454 Venoy Rd, Wayne MI 48184).

**Revision 3:** Section II. RFP Specifications, A. Program Requirements Table:

|  |  |
| --- | --- |
| **Quantity** | **Item** |
| ~~19~~ **3** | 25’ SQUARE STEEL POLE RAB PS4-11-25D2 OR EQUAL (SEE ATTACHED SPECS) |
| ~~19~~ **3** | LED FIXTURE RAB LOT3T160/D10 OR EQUAL (SEE ATTATCHED SPECS) |
| ~~2~~ **8** | 15’ SQUARE STEEL POLE RAB PS4-11-15D2 OR EQUAL (SEE ATTACHED SPECS) |
| ~~2~~ **8** | LED FIXTURE RAB LOT3T110/D10 OR EQUAL (SEE ATTATCHED SPECS) |

**Poles 1 – 8 on the map in Appendix 1 should be 15’. Poles 9 – 11 on the map in Appendix 1 should be 25’.**

**Q.1.** It states the type of resulting contract is a Statewide Cooperative Contract. Is this true?

**A.1.** No, this is not a Statewide Cooperative Contract and the language should be removed.

**Q.2.** Please provide the panel location that will be utilized to provide power to the new light poles.

**A.2.** The vendor will need to visit the location to determine this.

**Q.3.** Will power be coming from the same panel as the existing lighting?

**A.3.** Yes, but the vendor will need to verify.

**Q.4.** Can existing conduit be reused or will all new conduit be required?

**A.4.** New conduit will be required.

**Q.5.** Please provide the number of circuits that will be required for the new lighting.

**A.5.** The vendor will need to visit the location to determine this.

**Q.6.** Does the existing panel that will be utilized for the new lighting have sufficient spare breakers?

**A.6.** The vendor will need to visit the location to determine this.

**Q.7.** Existing poles #4, #5, #6, #7, #8 have 2 heads per pole and the count shows only 1 per pole.

**A.7.** The existing poles and heads may be different than what is being requested to replace them.

**Q.8.** Can the existing conduit and existing wire be abandoned below grade?

**A.8.** Yes, it can be abandoned as long as the site clean up is complete.